Open topic with navigation

Disconnected: You’re looking at a local copy of the Appliance Controller Documentation Center. The most current version is online at www.quantum.com/accdocs.

# Refresh NAS Authentication Mappings

You can refresh your NAS authentication mappings on-demand to reflect the current state of your LDAP server. By performing this refresh, you will be refreshing ID map cache. In addition, this refresh is performed without restarting SMB services, so client connections persist.

Note: For a list of all the Appliance Controller commands, see the Command Index.

1. Log in to the Appliance Controller CLI.
2. Enter:

   auth refresh

   Example:

   > auth refresh

   Refresh auth configuration starting ...

   Broadcasting auth-refresh to NAS cluster ...

   Clearing ID map cache ...

   Waiting for auth_refresh to complete on node 10.65.190.xxx

   [10.65.190.xxx]: Request from 10.65.191.xx to refresh auth configuration startin g ...

   [10.65.190.xxx]: Clearing ID map cache ...

   Waiting for auth_refresh to complete on node 10.65.173.xxx

   [10.65.173.xxx]: Request from 10.65.191.xx to refresh auth configuration startin g ...

   [10.65.173.xxx]: Clearing ID map cache ...

   Successfully refreshed configuration services

6-68456-07_RevA | Initial publication date: Friday, December 22, 2017 | Last updated on Monday, January 12, 2026.

Open topic with navigation