Open topic with navigation

Disconnected: You’re looking at a local copy of the Appliance Controller Documentation Center. The most current version is online at www.quantum.com/accdocs.

# Default MIBs

When you enable the Main SNMP services, default Management Information Base (MIB) files are automatically included in your SNMP configuration. The following sections list each of these default MIBs and their corresponding object identifiers (OIDs).

Note: For a list of all the Appliance Controller commands, see the Command Index.

## MIB File Location

All supported MIB files are located in the following directory:

/usr/share/snmp/mibs

## What are MIBs and OIDs?

MIBs are a hierarchical database of OIDs, which form a data tree. Starting at the root, each OID travels along earlier nodes to its final node, which provides its value.

Example

In the following table, the snaAdDomIndex, snaAdDomName, and snaAdDomClusters OIDs are next generations of the snaAdDomEntry OID.

Name | OID | Description
--- | --- | ---
snaAdDomEntry | .1.3.6.1.4.1.3697.1.50.1.1.31.1 | Administrative Domain
snaAdDomIndex | .1.3.6.1.4.1.3697.1.50.1.1.31.1.1 | Index assigned to administrative domain
snaAdDomName | .1.3.6.1.4.1.3697.1.50.1.1.31.1.2 | Name of administrative domain
snaAdDomClusters | .1.3.6.1.4.1.3697.1.50.1.1.31.1.3 | Comma separated list of clusters in administrative domain

Default UCD SNMP MIB

When you enable the Main SNMP service, your system will respond to a limited set of Standard UCD SNMP queries about the operating system. The default MIB associated with these queries is detailed in the following table.

Note: When the SNMP service is enabled, SNMP is granted read-only access on the standard SNMP UDP Port 161.

Table 1: Default UCD SNMP MIB
Name | OID | Description
--- | --- | ---
System Information | .1.3.6.1.2.1.1 | System description System uptime System contact System name System location System services ...
Interfaces | .1.3.6.1.2.1.2.0.0.2 | SNMP MIB-2 Interfaces
Networking | .1.3.6.1.2.1.4 | IP forwarding IP default TTL IP in receives IP in address errors IP route table ...
Load Statistics | .1.3.6.1.4.1.2021.10 | Load average Names Load Config ...
CPU Statistics | .1.3.6.1.4.1.2021.11 | System statistics CPU system CPU idle Swap in swap out IO sent Interrupts ...
Memory Statistics | .1.3.6.1.4.1.2021.4 | Real available Swap errors Total free Minimum swap Shared buffer Cached Total swap Available swap Total real Available real ...
Disk Statistics | .1.3.6.1.4.1.2021.9 | Total Available Used Path Device ...

Default StorNext SNMP MIB

When you enable the StorNext SNMP agent, your system will respond to over 100 SNMP queries about the StorNext file system. These queries are defined by the default StorNext SNMP MIB file's .1.3.6.1.4.1.3697.1.50 OID tree.

Each of the following tables details the nodes within the .1.3.6.1.4.1.3697.1.50 OID tree.

Table 2: Overall Parameters
Name | OID | Description
--- | --- | ---
snaDescription | .1.3.6.1.4.1.3697.1.50.1.1.1 | Description of the StorNext appliance
snaFileSystemServerVersion | .1.3.6.1.4.1.3697.1.50.1.1.2 | File system server verions
snaFileSystemClientVersion | .1.3.6.1.4.1.3697.1.50.1.1.3 | File system client version
snaGatewayAgentVersion | .1.3.6.1.4.1.3697.1.50.1.1.4 | Gateway agent version
snaPlatform | .1.3.6.1.4.1.3697.1.50.1.1.5 | Platform of the StorNext appliance
snaSerialNumber | .1.3.6.1.4.1.3697.1.50.1.1.6 | Serial Number of the StorNext appliance
snaStateHostNodeNumber | .1.3.6.1.4.1.3697.1.50.1.1.22 | State of Node number of the StorNext host
snaHostNodeNumber | .1.3.6.1.4.1.3697.1.50.1.1.23 | Node number of the StorNext host

Table 3: StorNext Health
Name | OID | Description
--- | --- | ---
snaOnlineState | .1.3.6.1.4.1.3697.1.50.1.1.10 | Overall StorNext Appliance online status
snaStateNumberOfOpenRASTickets | .1.3.6.1.4.1.3697.1.50.1.1.11 | State of the value given as number of open RAS Tickets
snaNumberOfOpenRASTickets | .1.3.6.1.4.1.3697.1.50.1.1.12 | Number of open RAS Tickets
snaStateNumberOfAdminAlerts | .1.3.6.1.4.1.3697.1.50.1.1.13 | State of the value given as number of Admin Alerts
snaNumberOfAdminAlerts | .1.3.6.1.4.1.3697.1.50.1.1.14 | Number of Admin Alerts
snaPriorOnlineState | .1.3.6.1.4.1.3697.1.50.1.1.25 | Overall StorNext Appliance online status from prior poll period
snaPriorNumberOfOpenRASTickets | .1.3.6.1.4.1.3697.1.50.1.1.26 | Number of open RAS Tickets from prior poll period

Table 4: Administrative Domains
Name | OID | Description
--- | --- | ---
snaNumberOfAdDoms | .1.3.6.1.4.1.3697.1.50.1.1.30 | Number of administrative domains
snaAdDomTable | .1.3.6.1.4.1.3697.1.50.1.1.31 | Administrative domain table
snaAdDomEntry | .1.3.6.1.4.1.3697.1.50.1.1.31.1 | Administrative Domain
Administrative Domain Table Entries
snaAdDomIndex | .1.3.6.1.4.1.3697.1.50.1.1.31.1.1 | Index assigned to administrative domain
snaAdDomName | .1.3.6.1.4.1.3697.1.50.1.1.31.1.2 | Name of administrative domain
snaAdDomClusters | .1.3.6.1.4.1.3697.1.50.1.1.31.1.3 | Comma separated list of clusters in administrative domain

Table 5: Clusters
Name | OID | Description
--- | --- | ---
snaNumberOfClusters | .1.3.6.1.4.1.3697.1.50.1.1.40 | Number of clusters
snaClusterTable | .1.3.6.1.4.1.3697.1.50.1.1.41 | Cluster table
snaClusterEntry | .1.3.6.1.4.1.3697.1.50.1.1.41.1 | Cluster
Cluster Table Entries
snaClusterIndex | .1.3.6.1.4.1.3697.1.50.1.1.41.1.1 | Index assigned to cluster
snaClusterName | .1.3.6.1.4.1.3697.1.50.1.1.41.1.2 | Name of cluster
snaClusterAdDomName | .1.3.6.1.4.1.3697.1.50.1.1.41.1.3 | Name of administrative domain containing this cluster
snaClusterFileSystems | .1.3.6.1.4.1.3697.1.50.1.1.41.1.4 | Comma separated list of file systems in cluster

Table 6: File Systems
Name | OID | Description
--- | --- | ---
snaNumberOfFileSystems | .1.3.6.1.4.1.3697.1.50.1.1.50 | Number of file systems
snaFileSystemTable | .1.3.6.1.4.1.3697.1.50.1.1.51 | File system table
snaFileSystemEntry | .1.3.6.1.4.1.3697.1.50.1.1.51.1 | File System
File System Table Entries
snaFileSystemIndex | .1.3.6.1.4.1.3697.1.50.1.1.51.1.1 | Index assigned to file system
snaFileSystemName | .1.3.6.1.4.1.3697.1.50.1.1.51.1.2 | Name of file system
snaFileSystemClusterName | .1.3.6.1.4.1.3697.1.50.1.1.51.1.3 | Name of cluster containing this file system
snaFileSystemAdDomName | .1.3.6.1.4.1.3697.1.50.1.1.51.1.4 | Name of the administrative domain containing this file system
snaFileSystemHost | .1.3.6.1.4.1.3697.1.50.1.1.51.1.5 | Host for this file system
snaFileSystemAddr | .1.3.6.1.4.1.3697.1.50.1.1.51.1.6 | Network IP address for this file system
snaFileSystemPort | .1.3.6.1.4.1.3697.1.50.1.1.51.1.7 | Network IP port for this file system
snaFileSystemActive | .1.3.6.1.4.1.3697.1.50.1.1.51.1.8 | Whether this file system is active
snaFileSystemHaShared | .1.3.6.1.4.1.3697.1.50.1.1.51.1.9 | Whether this file is high-availability shared
snaFileSystemMkFsTime | .1.3.6.1.4.1.3697.1.50.1.1.51.1.10 | Date and time when this file system was created
snaFileSystemFsID | .1.3.6.1.4.1.3697.1.50.1.1.51.1.11 | This file system's identifier
snaFileSystemSize | .1.3.6.1.4.1.3697.1.50.1.1.51.1.12 | Total size of the file system
snaFileSystemFree | .1.3.6.1.4.1.3697.1.50.1.1.51.1.13 | Size of free area in file system
snaFileSystemBlockSize | .1.3.6.1.4.1.3697.1.50.1.1.51.1.14 | Block size for file system
snaFileSystemConnections | .1.3.6.1.4.1.3697.1.50.1.1.51.1.15 | Number of connections to file system
snaFileSystemManaged | .1.3.6.1.4.1.3697.1.50.1.1.51.1.16 | Whether file system is managed
snaFileSystemQuotas | .1.3.6.1.4.1.3697.1.50.1.1.51.1.17 | Whether file system uses quotas
snaFileSystemQos | .1.3.6.1.4.1.3697.1.50.1.1.51.1.18 | Whether file system uses quality of service
snaFileSystemFiles | .1.3.6.1.4.1.3697.1.50.1.1.51.1.19 | Number of files in file system
snaFileSystemDirectories | .1.3.6.1.4.1.3697.1.50.1.1.51.1.20 | Number of directories in file system

Table 7: Stripe Groups
Name | OID | Description
--- | --- | ---
snaNumberOfStripeGroups | .1.3.6.1.4.1.3697.1.50.1.1.61.0 | Number of stripe group
snaSripeGroupTable | .1.3.6.1.4.1.3697.1.50.1.1.61 | Stripe group table
snaStripeGroupEntry | .1.3.6.1.4.1.3697.1.50.1.1.61.1 | Stripe Group
Stripe Group Table Entries
snaStripeGroupIndex | .1.3.6.1.4.1.3697.1.50.1.1.61.1.1 | Index assigned to stripe group
snaStripeGroupName | .1.3.6.1.4.1.3697.1.50.1.1.61.1.2 | Name of stripe group
snaStripeGroupFileSystemName | .1.3.6.1.4.1.3697.1.50.1.1.61.1.3 | Name of the containing file system
snaStripeGroupClusterName | .1.3.6.1.4.1.3697.1.50.1.1.61.1.4 | Name of the containing cluster
snaStripeGroupAdDomName | .1.3.6.1.4.1.3697.1.50.1.1.61.1.5 | Name of the containing administrative domain
snaStripeGroupEnabled | .1.3.6.1.4.1.3697.1.50.1.1.61.1.6 | Whether the stripe group is enabled
snaStripeGroupMetadata | .1.3.6.1.4.1.3697.1.50.1.1.61.1.7 | Whether the stripe group has metadata
snaStripeGroupJournal | .1.3.6.1.4.1.3697.1.50.1.1.61.1.8 | Whether the stripe group is journaling
snaStripeGroupExclusive | .1.3.6.1.4.1.3697.1.50.1.1.61.1.9 | Whether the stripe group is exclusive
snaStripeGroupBreadth | .1.3.6.1.4.1.3697.1.50.1.1.61.1.10 | Breadth of the stripe group
snaStripeGroupSize | .1.3.6.1.4.1.3697.1.50.1.1.61.1.11 | Size of the stripe group
snaStripeGroupReserved | .1.3.6.1.4.1.3697.1.50.1.1.61.1.12 | Size of the reserved area in the stripe group
snaStripeGroupFree | .1.3.6.1.4.1.3697.1.50.1.1.61.1.13 | Size of the free area in the stripe group
snaStripeGroupDisks | .1.3.6.1.4.1.3697.1.50.1.1.61.1.14 | Comma separated list of disks in stripe group

Table 8: Clients
Name | OID | Description
--- | --- | ---
snaNumberOfClients | .1.3.6.1.4.1.3697.1.50.1.1.70 | Number of StorNext clients for active file system
snaClientTable | .1.3.6.1.4.1.3697.1.50.1.1.71 | StorNext client table
snaClientEntry | .1.3.6.1.4.1.3697.1.50.1.1.71.1 | StorNext client
Client Table Entries
snaClientIndex | .1.3.6.1.4.1.3697.1.50.1.1.71.1.1 | Index assigned to StorNext client
snaClientHost | .1.3.6.1.4.1.3697.1.50.1.1.71.1.2 | Client host name
snaClientFileSystemName | .1.3.6.1.4.1.3697.1.50.1.1.71.1.3 | File system used by client
snaClientClusterName | .1.3.6.1.4.1.3697.1.50.1.1.71.1.4 | Cluster for file system used by client
snaClientAdDomName | .1.3.6.1.4.1.3697.1.50.1.1.71.1.5 | Administrative domain for file system used by client
snaClientAddr | .1.3.6.1.4.1.3697.1.50.1.1.71.1.6 | Network IP address of client
snaClientUpTime | .1.3.6.1.4.1.3697.1.50.1.1.71.1.7 | Time that client has been up
snaClientLicExpiry | .1.3.6.1.4.1.3697.1.50.1.1.71.1.8 | Client license expiration
snaClientReconnects | .1.3.6.1.4.1.3697.1.50.1.1.71.1.9 | Number of times client has reconnected
snaClientDlcGateway | .1.3.6.1.4.1.3697.1.50.1.1.71.1.10 | Whether DLC gateway
snaClientDlcGatewayLicense | .1.3.6.1.4.1.3697.1.50.1.1.71.1.11 | Whether DLC gateway license
snaClientDlcClient | .1.3.6.1.4.1.3697.1.50.1.1.71.1.12 | Whether DLC client
snaClientDlcHybridClient | .1.3.6.1.4.1.3697.1.50.1.1.71.1.13 | Whether DLC hybrid client

Table 9: Coordinators
Name | OID | Description
--- | --- | ---
snaNumberOfCoordinators | .1.3.6.1.4.1.3697.1.50.1.1.80 | Number of coordinators
snaCoordTable | .1.3.6.1.4.1.3697.1.50.1.1.81 | Coordinator table
snaCoordEntry | .1.3.6.1.4.1.3697.1.50.1.1.81.1 | Coordinator
Coordinator Table Entries
snaCoordIndex | .1.3.6.1.4.1.3697.1.50.1.1.81.1.1 | Index assigned to coordinator
snaCoordName | .1.3.6.1.4.1.3697.1.50.1.1.81.1.2 | Name of coordinator
snaCoordAddr | .1.3.6.1.4.1.3697.1.50.1.1.81.1.3 | Network IP address of coordinator

Table 10: Hosts
Name | OID | Description
--- | --- | ---
snaNumberOfHosts | .1.3.6.1.4.1.3697.1.50.1.1.100 | Number of hosts
snaHostTable | .1.3.6.1.4.1.3697.1.50.1.1.101 | Host table
snaHostEntry | .1.3.6.1.4.1.3697.1.50.1.1.101.1 | Host
Host Table Entries
snaHostIndex | .1.3.6.1.4.1.3697.1.50.1.1.101.1.1 | Index assigned to host
snaHostName | .1.3.6.1.4.1.3697.1.50.1.1.101.1.2 | Name of host
snaHostIpAddress | .1.3.6.1.4.1.3697.1.50.1.1.101.1.3 | Network IP address of host
snaHostHostStatus | .1.3.6.1.4.1.3697.1.50.1.1.101.1.4 | Host status
snaFsRelease | .1.3.6.1.4.1.3697.1.50.1.1.101.1.5 | Host file system release
snaFsMajor | .1.3.6.1.4.1.3697.1.50.1.1.101.1.6 | Host file system major version number
snaFsMinor | .1.3.6.1.4.1.3697.1.50.1.1.101.1.7 | Host file system minor version number
snaFsRel | .1.3.6.1.4.1.3697.1.50.1.1.101.1.8 | Host file system release version number
snaFsReleaseRev | .1.3.6.1.4.1.3697.1.50.1.1.101.1.9 | Host file system revision version number
snaHaPrimary | .1.3.6.1.4.1.3697.1.50.1.1.101.1.10 | Whether Host is the high availability primary host
snaApplianceSerialNumber | .1.3.6.1.4.1.3697.1.50.1.1.101.1.11 | Host appliance serial number
snaApplianceManufacturer | .1.3.6.1.4.1.3697.1.50.1.1.101.1.12 | Host appliance manufacturer
snaApplianceBuildYear | .1.3.6.1.4.1.3697.1.50.1.1.101.1.13 | Host appliance build year
snaApplianceBuildWeek | .1.3.6.1.4.1.3697.1.50.1.1.101.1.14 | Host appliance build week within year
snaApplianceModel | .1.3.6.1.4.1.3697.1.50.1.1.101.1.15 | Host appliance model
snaApplianceNumber | .1.3.6.1.4.1.3697.1.50.1.1.101.1.16 | Host appliance number
snaOsVersion | .1.3.6.1.4.1.3697.1.50.1.1.101.1.17 | Host operating system version
snaFsNameHost | .1.3.6.1.4.1.3697.1.50.1.1.101.1.18 | Whether this host is acting as a network name host
snaHaNode | .1.3.6.1.4.1.3697.1.50.1.1.101.1.19 | Whether this host is a high availability node
snaHaEnabled | .1.3.6.1.4.1.3697.1.50.1.1.101.1.20 | Whether this host has high availability enabled
snaHaPeerIp | .1.3.6.1.4.1.3697.1.50.1.1.101.1.21 | The network IP address of this hosts's high availability peer
snaFsBuild | .1.3.6.1.4.1.3697.1.50.1.1.101.1.22 | Host file system build information
snaFsTarget | .1.3.6.1.4.1.3697.1.50.1.1.101.1.23 | Host file system target information
snaFsDate | .1.3.6.1.4.1.3697.1.50.1.1.101.1.24 | Host file system build date
snaFsDir | .1.3.6.1.4.1.3697.1.50.1.1.101.1.25 | Host file system build directory
snaFsBranch | .1.3.6.1.4.1.3697.1.50.1.1.101.1.26 | Host file system build branch
snaFsBuildId | .1.3.6.1.4.1.3697.1.50.1.1.101.1.27 | Host file system build identifier
snaCpus | .1.3.6.1.4.1.3697.1.50.1.1.101.1.28 | Number of central processing units in host
snaMdc | .1.3.6.1.4.1.3697.1.50.1.1.101.1.29 | Whether this is a metadata controller

Table 11: Host Disks
Name | OID | Description
--- | --- | ---
snaNumberOfHostDisks | .1.3.6.1.4.1.3697.1.50.1.1.110 | Number of host disks
snaHostDiskTable | .1.3.6.1.4.1.3697.1.50.1.1.111 | Host Disk table
snaHostDiskEntry | .1.3.6.1.4.1.3697.1.50.1.1.111.1 | Host Disk
Host Disk Table Entries
snaHostDiskIndex | .1.3.6.1.4.1.3697.1.50.1.1.111.1.1 | Index assigned to Host Disk
snaHostDiskName | .1.3.6.1.4.1.3697.1.50.1.1.111.1.2 | Name of host disk
snaHostDiskHostName | .1.3.6.1.4.1.3697.1.50.1.1.111.1.3 | Name of Host on which disk is attached

Table 12: Host Services
Name | OID | Description
--- | --- | ---
snaNumberOfHostServices | .1.3.6.1.4.1.3697.1.50.1.1.120 | Number of host services
snaHostServiceTable | .1.3.6.1.4.1.3697.1.50.1.1.121 | Host service table
snaHostServiceEntry | .1.3.6.1.4.1.3697.1.50.1.1.121.1 | Host service
Host Service Table Entries
snaHostServiceIndex | .1.3.6.1.4.1.3697.1.50.1.1.121.1.1 | Index assigned to host service
snaHostServiceName | .1.3.6.1.4.1.3697.1.50.1.1.121.1.2 | Name of host service
snaHostServiceHostName | .1.3.6.1.4.1.3697.1.50.1.1.121.1.3 | Name of Host on which service is running
snaHostServicePort | .1.3.6.1.4.1.3697.1.50.1.1.121.1.4 | Network port used by host service
snaHostServicePid | .1.3.6.1.4.1.3697.1.50.1.1.121.1.5 | Process identifier of host service
snaHostServiceStateChange | .1.3.6.1.4.1.3697.1.50.1.1.121.1.6 | Date and time of last state change of host service
snaHostServiceNumberLaunches | .1.3.6.1.4.1.3697.1.50.1.1.121.1.7 | Number of launches of host service
snaHostServiceNumberCoreDumps | .1.3.6.1.4.1.3697.1.50.1.1.121.1.8 | Number of core dumps of host service

Table 13: Host File Systems
Name | OID | Description
--- | --- | ---
snaNumberOfHostFileSystems | .1.3.6.1.4.1.3697.1.50.1.1.130 | Number of host file systems
snaHostFileSystemTable | .1.3.6.1.4.1.3697.1.50.1.1.131 | Host File System table
snaHostFileSystemEntry | s.1.3.6.1.4.1.3697.1.50.1.1.131.1 | s Host File System
Host File System Table Entries
snaHostFileSystemIndex | .1.3.6.1.4.1.3697.1.50.1.1.131.1.1 | Index assigned to Host File System
snaHostFileSystemName | .1.3.6.1.4.1.3697.1.50.1.1.131.1.2 | Name of host file system
snaHostFileSystemHostName | .1.3.6.1.4.1.3697.1.50.1.1.131.1.3 | Name of Host on which file system is running

Table 14: Host File System Mounts
Name | OID | Description
--- | --- | ---
snaNumberOfHostFsMounts | .1.3.6.1.4.1.3697.1.50.1.1.140 | Number of host file system mounts
snaHostFsMountTable | .1.3.6.1.4.1.3697.1.50.1.1.141 | Host File System Mount table
snaHostFsMountEntry | .1.3.6.1.4.1.3697.1.50.1.1.141.1 | Host File System Mount
Host File System Mount Table Entries
snaHostFsMountIndex | .1.3.6.1.4.1.3697.1.50.1.1.141.1.1 | Index assigned to Host File System
snaHostFsMountName | .1.3.6.1.4.1.3697.1.50.1.1.141.1.2 | Name of host file system mount
snaHostFsMountHostName | .1.3.6.1.4.1.3697.1.50.1.1.141.1.3 | Name of Host on which file system is mounted

Table 15: Host Licenses
Name | OID | Description
--- | --- | ---
snaNumberOfHostLicenses | .1.3.6.1.4.1.3697.1.50.1.1.150 | Number of host file system licenses
snaHostLicenseTable | .1.3.6.1.4.1.3697.1.50.1.1.151 | Host File System License table
snaHostLicenseEntry | .1.3.6.1.4.1.3697.1.50.1.1.151.1 | Host File System License
Host License Table Entries
snaHostLicenseIndex | .1.3.6.1.4.1.3697.1.50.1.1.151.1.1 | Index assigned to Host License
snaHostLicenseName | .1.3.6.1.4.1.3697.1.50.1.1.151.1.2 | Name of host license
snaHostLicenseHostName | 1.3.6.1.4.1.3697.1.50.1.1.151.1.3 | Name of Host for license
snaHostLicenseCapacity | .1.3.6.1.4.1.3697.1.50.1.1.151.1.4 | Number of licensed entities or 0 if unlimited or irrelevant
snaHostLicenseExpiry | .1.3.6.1.4.1.3697.1.50.1.1.151.1.5 | Host license expiration

Table 16: Disks
Name | OID | Description
--- | --- | ---
snaNumberOfDisks | .1.3.6.1.4.1.3697.1.50.1.1.160 | Number of disks
snaDiskTable | .1.3.6.1.4.1.3697.1.50.1.1.161 | Disk table
snaDiskEntry | .1.3.6.1.4.1.3697.1.50.1.1.161.1 | Disk
Disk Table Entries
snaDiskIndex | .1.3.6.1.4.1.3697.1.50.1.1.161.1.1 | Index assigned to disk
snaDiskName | .1.3.6.1.4.1.3697.1.50.1.1.161.1.2 | Name of disk
snaDiskSize | .1.3.6.1.4.1.3697.150.1.1.161.1.3 | Size of the disk
snaDiskSector | .1.3.6.1.4.1.3697.150.1.1.161.1.4 | Sector of the disk
snaDiskHosts | .1.3.6.1.4.1.3697.150.1.1.161.1.5 | Comma separated list of hosts using this disk
snaDiskInquiry | .1.3.6.1.4.1.3697.150.1.1.161.1.6 | Disk inquiry
snaDiskController | .1.3.6.1.4.1.3697.150.1.1.161.1.7 | Disk controller
snaDiskSerial | .1.3.6.1.4.1.3697.150.1.1.161.1.8 | Disk serial number

Table 17: Disk Types
Name | OID | Description
--- | --- | ---
snaNumberOfDiskTypes | .1.3.6.1.4.1.3697.1.50.1.1.170 | Number of disk types
snaDiskTypeTable | .1.3.6.1.4.1.3697.1.50.1.1.171 | Disk type table
snaDiskTypeEntry | .1.3.6.1.4.1.3697.1.50.1.1.171.1 | Disk Type
Disk Type Table Entries
snaDiskTypeIndex | .1.3.6.1.4.1.3697.1.50.1.1.171.1.1 | Index assigned to disk type
snaDiskTypeClass | .1.3.6.1.4.1.3697.1.50.1.1.171.1.2 | Class of disk type
snaDiskTypeSize | .1.3.6.1.4.1.3697.150.1.1.171.1.3 | Size of the disk type
snaDiskTypeCount | .1.3.6.1.4.1.3697.150.1.1.171.1.4 | Number of disks on this type

Table 18: Notifications
Name | OID | Description
--- | --- | ---
SNMPv2c Trap: snaNotifyStatusChange | 1.3.6.1.4.1.3697.1.50.1.4.1.1 | Notification that the StorNext Appliance number of open RAS tickets has increased.
Argument: snaNumberOfOpenRASTickets | .1.3.6.1.4.1.3697.1.50.1.1.12 | Number of open RAS Tickets.
Argument: snaPriorNumberOfOpenRASTickets | .1.3.6.1.4.1.3697.1.50.1.1.26 | Number of open RAS Tickets from prior poll period.
SNMPv2c Trap: snaNotifyOnlineStateChange | .1.3.6.1.4.1.3697.1.50.1.4.1.2 | Notification that the StorNext Appliance online state has changed.
Argument: snaOnlineState | .1.3.6.1.4.1.3697.1.50.1.1.10 | Overall StorNext Appliance online status.
Argument: snaPriorOnlineState | .1.3.6.1.4.1.3697.1.50.1.1.25 | Overall StorNext Appliance online status from prior poll period.

Default Dell OpenManage MIBs

When you enable the Dell OpenManage agent, the system will respond to hundreds of SNMP queries. Two default OpenManage MIB files and OIDs associated with these queries are detailed in the following tables.

Table 19: Systems Management Instrumentation MIB
Name | OID | Description
--- | --- | ---
system | .1.3.6.1.2.1.1.1 | System Description
health | .1.3.6.1.4.1.674.10892.1.200.10.1.2.1 | System status
chassis health | .1.3.6.1.4.1.674.10892.1.200.10.1.4.1 | Chassis health
processor health | .1.3.6.1.4.1.674.10892.1.200.10.1.50.1 | Processor health
power health | .1.3.6.1.4.1.674.10892.1.200.10.1.9.1 | Power system status
cooling health | .1.3.6.1.4.1.674.10892.1.200.10.1.21.1 | Cooling health
memory health | .1.3.6.1.4.1.674.10892.1.200.10.1.27.1 | Memory health
event log health | .1.3.6.1.4.1.674.10892.1.200.10.1.41.1 | Event log health
power redundancy | .1.3.6.1.4.1.674.10892.1.200.10.1.9.1 | Power redundancy status
network devices | .1.3.6.1.4.1.674.10892.1.1100.90.1.5.1 | Network device names
cooling devices | .1.3.6.1.4.1.674.10892.1.700.12.1.8.1 | Cooling device locations

Table 20: Server Administrator Storage Management MIB
Name | OID | Description
--- | --- | ---
disks | .1.3.6.1.4.1.674.10893.1.20.130.4.1.2 | Disks
storage health | .1.3.6.1.4.1.674.10893.1.20.2 | Storage health
storage agent health | .1.3.6.1.4.1.674.10893.1.20.110.13 | Storage management agent health rollup
storage controller | .1.3.6.1.4.1.674.10893.1.20.130.1.1.2.1 | Storage controller name
storage controller type | .1.3.6.1.4.1.674.10893.1.20.130.1.1.4.1 | Storage controller type
storage controller state | .1.3.6.1.4.1.674.10893.1.20.130.1.1.5.1 | Storage controller state
storage controller fw | .1.3.6.1.4.1.674.10893.1.20.130.1.1.8.1 | Storage controller firmware version
storage controller cache | .1.3.6.1.4.1.674.10893.1.20.130.1.1.9.1 | Storage controller cache size
storage controller number | .1.3.6.1.4.1.674.10893.1.20.130.1.1.11.1 | Number of storage controller devices
storage controller vd | .1.3.6.1.4.1.674.10893.1.20.130.1.1.12.1 | Number of virtual disks on the controller
storage controller health | .13.6.1.4.1.674.10893.1.20.130.1.1.37.1 | Combined health of storage controller and its components
storage controller component health | .1.3.6.1.4.1.674.10893.1.20.130.1.1.38.1 | Health of storage controller itself without the propagation of any contained component status
storage controller alarm state | .1.3.6.1.4.1.674.10893.1.20.130.1.1.40.1 | Alarm state or setting for the storage controller
storage controller driver version | .1.3.6.1.4.1.674.10893.1.20.130.1.1.41.1 | Driver version of storage controller
storage controller slot | .1.3.6.1.4.1.674.10893.1.20.130.1.1.42.1 | PIC slot or embedded number for motherboard of storage controller
storage controller channels | .1.3.6.1.4.1.674.10893.1.20.130.1.1.47.1 | Channel count of the storage controller
storage controller channel state | .1.3.6.1.4.1.674.10893.1.20.130.2.1.7.1 | Channel name and state for channel on the storage controller

6-68456-07_RevA | Initial publication date: Friday, December 22, 2017 | Last updated on Monday, January 12, 2026.

Open topic with navigation