Open topic with navigation

Disconnected: You’re looking at a local copy of the Appliance Controller Documentation Center. The most current version is online at www.quantum.com/accdocs.

# Enable SNMP Authorization Traps

An authentication failure trap is an asynchronous message sent from a managed device, notifying the SNMP manager that someone has attempted to use the wrong community string or other authentication string.

You can enable SNMP agents to send authentication failure traps to the SNMP manager. The default setting is to have SNMP authorization traps disabled.

Note: For a list of all the Appliance Controller commands, see the Command Index.

1. Log in to the Appliance Controller CLI.
2. Enter:

snmp authtrapenable (enable | disable)

The parameter is:

`(enable | disable)` | Enter`enable` to enable SNMP authorization traps. Enter`disable` to disable SNMP authorization traps. Note: The default setting is to have SNMP authorization traps disabled.

6-68456-07_RevA | Initial publication date: Friday, December 22, 2017 | Last updated on Monday, January 12, 2026.

Open topic with navigation