Open topic with navigation

Disconnected: You’re looking at a local copy of the Appliance Controller Documentation Center. The most current version is online at www.quantum.com/accdocs.

# View System Status

You can view your Appliance Controller system's status to determine which of the following features are configured and running.

System Features

The `system status` command reports on the following features.

Feature | Description
--- | ---
`snnas_controller` | The state of the Appliance Controller. The controller state should always be `running`.
`ctdb` | The state of the clustered trivial database (ctdb). This process manages the lock state for the SMB cluster. If the Samba server daemon (smbd) is disabled or is not running within a NAS cluster, then the ctdb state is `disabled`. If smbd is running within a NAS cluster, then the ctdb state is `running`.
`smbd` | The state of the smbd process. The typical smbd state is `running`. If the smbd process has been disabled (with the `nas smb disable` command), then the smbd state is `disabled`.
`winbind` | The state of the winbind binding process. If local user-authentication is configured, then the winbind state is `disabled`. If AD or LDAP user-authentication is configured, then the winbind state is `running`.
`nfs` | The state of the NFS server daemon process. The typical nfs state is `running`. If the nfs process has been disabled (with the `nas nfs disable` command), then the nfs state is `disabled`.
`haproxy` | The state of the haproxy process. This process is only applicable to a NAS cluster of Xcellis WFE or G300 gateways — it manages the load balancing between the cluster's nodes. If the system is not part of a NAS cluster or if the node being checked is not the master node, then the haproxy state is `disabled`. If the system is part of a NAS cluster and the node being checked is the master node, then the haproxy state is `running`.
`keepalived` | The state of the keepalived process. This process manages the VIP movement from one node to another during NAS failover. If the system is not part of a NAS cluster, then the keepalived state is `disabled`. If the system is part of a NAS cluster, then the keepalived state is `running`.
`snmpd` | The state of the Simple Network Management Protocol (SNMP) daemon process. See SNMP Monitoring for additional information. The typical SNMP state is `disabled`.

View System Status

1. Log in to the Appliance Controller CLI.
2. Enter:

   system status all

   The parameter is:

   `all` | Enter `all` to view the status of all system services. Otherwise, only the status of the Appliance Controller is returned.

Example output:

    snnas_controller: running
                ctdb: running
                smbd: running
             winbind: running
                 nfs: running
             haproxy: disabled
          keepalived: running
               snmpd: disabled

6-68456-07_RevA | Initial publication date: Friday, December 22, 2017 | Last updated on Monday, January 12, 2026.

Open topic with navigation