Open topic with navigation

Disconnected: You’re looking at a local copy of the Appliance Controller Documentation Center. The most current version is online at www.quantum.com/accdocs.

# View SNMP Service Configuration

Before completing the configuration of your SNMP services, you can view all or selected parts of the SNMP service configuration that will be written to the `snmpd.conf` file.

Note: For a list of all the Appliance Controller commands, see the Command Index.

1. Log in to the Appliance Controller CLI.
2. Enter:

   snmp show [service, sysinfo, community, view, trapcommunity, authtrapenable]

   The optional parameters are:

   `service` | Enter to query whether the service is enabled or disabled. See Enable or Disable SNMP Services.
   `sysinfo` | Enter to query system information, such as the administrator and managing device. See Define SNMP Maintenance Information.
   `community` | Enter to query community information, such as community name and network settings. See Configure an SNMP Community .
   `view` | Enter to query views set up for the community. See Configure an SNMP Community .
   `trapcommunity` | Enter to query the trap community's name. See Configure an SNMP Community .
   `authtrapenable` | Enter to query whether the authtrapenable service is enabled. See Enable SNMP Authorization Traps.

   If you do not enter optional parameters, all of the above parameters will be queried.

   Example:

   > snmp show

   SNMP service is enabled

   Agents:

   default agent is enabled.

   open-manage agent is enabled.

   stornext agent is enabled.

   Views:

   # This is the system MIB which gives system information such as uptime

   view systemInfo included .1.3.6.1.2.1.1

   # This is the IF-MIB branch which gives info on interfaces

   view systemInfo included .1.3.6.1.2.1.2.0.0.0.2

   # This branch contains networking information

   view systemInfo included .1.3.6.1.2.1.4

   view systemInfo included .1.3.6.1.4.11.3697.1.50

   # UCD-SNMP-MIB system statistic for load

   view systemInfo included .1.3.6.1.4.1.2021.10

   # UCD-SNMP-MIB system statistic for CPU

   view systemInfo included .1.3.6.1.4.1.2021.11

   # UCD-SNMP-MIB system statistic for memory

   view systemInfo included .1.3.6.1.4.1.2021.4

   # UCD-SNMP-MIB system statistic for disks

   view systemInfo included .1.3.6.1.4.1.2021.9

   view systemInfo included .1.3.6.1.4.1.3697

   view systemInfo included .1.3.6.1.4.1.3697.1.50

   view systemInfo included .1.3.6.1.4.1.674.10892

   Communities:

   rocommunity unguessable default -V systemInfo

   Notifications:

   trapcommunity public

   authtrapenable is disabled

   trap2sink 10.40.162.134:162

   trap2sink 10.40.163.163:162

6-68456-07_RevA | Initial publication date: Friday, December 22, 2017 | Last updated on Monday, January 12, 2026.

Open topic with navigation